RedBoot> load -v -r -b 0x00218000 -m http -h 192.168.0.10 /~me/zImage-72xx-2of 4096K si
Inode-cache hash table entries: 2048 (order: 1, 8192 bytes)itialized
.6.21-tsdis
Non-
\o
Raw file loaded 0x00218000-0x0037cbb3, assumed entry at 0x00218000al TUN/TAP device driver, 1.6e in FL
Memory: 29312KB available (27
RedBoot> exec -c "console=ttyAM0,115200 root=/dev/usb0"om>me              FLASH addr  Mem 
Mount-cache hash ta
Using base address 0x00218000 and length 0x00164bb4CPU: Testing write buffer coherency: oket, IRQ 39, 
Uncompressing Linux....................................ily 16             

Built 4 zonelists.  Total pages: 8128z
NetWinder Floating Point Emulator V
Kernel command line: console=ttyAM0,115200 root=/dev/usb0o devices on ID
mtd: pa
JFFS2 version 2.2. (NAND) (C) 200
PID hash table entries: 128 (order: 7, 512 bytes)> fis load vmlinux: "Re
yaffs Nov 15 2007 15:28:1
Console: colour dummy device 80x3000800000 : "FIS 
io scheduler noop
Dentry cache hash table entries: 4096 (order: 2, 16384 bytes)registered (default)8MB 8MB 8MB = 

RedBoo
ep93xx-ohci ep93xx
Inode-cache hash table entries: 2048 (order: 1, 8192 bytes)43K da
Gateway IP address: 192.168.0.1
Serial: AMBA driver $R
Memory: 8MB 8MB 8MB 8MB = 32MB totalio mem 0x80020000: ne
apb:uart1: tty
Memory: 29312KB available (2748K code, 254K data, 112K init)IRM920T) Rev A cache
Default se
usb usb
apb:uart2: ttyAM1 at
Mount-cache hash table entries: 512ARe
dns_ip: 192.168.0.123002000
us
CPU: Testing write buffer coherency: ok2 at MMIO 0x808e0000 (irq = 55) is a AM
NET: Registered protocol family 16h

         
io scheduler deadline registered (default)ain) (
Creating 4 MTD partitions on "physm
ep93xx_wdt: EP93XX watchdog, driver version 0.3........
NE
0x00000000-0x00620000 : "(reserved)
Serial: AMBA driver $Revision: 1.1.1.1 $0620000-0x00660000 : "RedBoot"..........
apb:uart1: ttyAM0 at MMIO 0x808c0000 (irq = 52) is a AMBAonfig"sion 0 (ARMv4T), cr=4
ieee80211: 802.11 
mtd: parti
apb:uart2: ttyAM1 at MMIO 0x808d0000 (irq = 54) is a AMBAce read-only SBC1: 802.11 data/
ieee80211: Copyright (C) 
apb:uart3: ttyAM2 at MMIO 0x808e0000 (irq = 55) is a AMBA : "FIS directory"Thu Nov 15            
CPU0: D VIVT wri
eth0: ep93xx on-chip ethernet, IRQ 39, 00:d0:69:40:2d:94.ot=" boot optiontivity 64, 
usb usb1: configuration #1 ch
Linux video capture interface: v2.00nable to mount root fs on un
hub 1-0
physmap platform flash device: 01000000 at 600000000:1.0: 3 ports detected line: cons

>> TS-BOOTROM,
physmap-flash.0: Found 1 x16 devices at 0x0 in 8-bit bank8192 bytes)512
PID has
usb 1-3: new full speed USB device
 Intel/Sharp Extended Query Table at 0x0031 total6 - bu
Conso
>> TS-7200: Rev E0 CPU, 
Using buffer write methodct: DataTraveler 2.0     
ep93xx-ohci ep93xx-ohci: irq 56, io mem 0x80020000t> fis load vmlinuxer: 0, 409
NET: Registered prot
usb usb1: Product: EP93xx OHCI8 2005      
RedB
ieee80211: 8
usb usb1: Manufacturer: Linux 2.6.21-ts ohci_hcdes)at, Inc.168.0.10 /~me/zImage-72xx-2
Can't
usb usb1: SerialNumber: ep93xx(C) 2004-2005 Intel Corporatio
usb usb1: configuration #1 chosen from 1 choice218000 -m http -h 192.168.0.10 /~test/zImage-
hub 1-0:1.0: USB hub found-m48t86: setting the syste
hub 1-0:1.0: 3 ports detected (12362481tsno regis
usb 1-3: configuration #1 chosen from 1 choice
scsi0 : SCSI emulation for USB Mass Storage devices
usbcore: registered new interface driver usb-storage
USB Mass Storage support registered.
usbcore: registered new interface driver usbhid
drivers/usb/input/hid-core.c: v2.6:USB HID core driver
mice: PS/2 mouse device common for all mice
rtc-m48t86 rtc-m48t86: rtc core: registered m48t86 as rtc0
rtc-m48t86 rtc-m48t86: battery ok
ep93xx-rtc ep93xx-rtc: rtc core: registered ep93xx as rtc1
TCP cubic registered
NET: Registered protocol family 1
NET: Registered protocol family 17
NET: Registered protocol family 15
ieee80211: 802.11 data/management/control stack, git-1.1.13
ieee80211: Copyright (C) 2004-2005 Intel Corporation <jketreno@linux.intel.com>
rtc-m48t86 rtc-m48t86: setting the system clock to 2009-03-05 10:22:15 (12362485
35)
Root-NFS: No NFS server available, giving up.
VFS: Unable to mount root fs via NFS, trying floppy.
VFS: Cannot open root device "usb0" or unknown-block(2,0)
Please append a correct "root=" boot option
Kernel panic - not syncing: VFS: Unable to mount root fs on unknown-block(2,0)